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Corrigendum

FINAL REPORT ON THE EVALUATION OF THE PILOT DEMONSTRATION PROJECTS ON ODS DISPOSAL AND DESTRUCTION

This corrigendum is being issued to:

· Replace Table 3 as follows:

	Country
	Type of ODS waste
	Amounts planned (mt)
	Amounts destroyed (mt)

	Colombia
	CFC-11 and CFC-12
	11 collected +103 estimated
	15.1 (domestic HTI)

	Georgia
	Various CFCs and HCFCs
	2.13 collected
	1.47 (export)

	Ghana
	CFC-12
	1.8 collected + 13 estimated 
	1.27 + 1.0 (export)

	Mexico
	Various CFCs and HCFCs
	119.7 collected + 47 estimated 
	74.1 (argon plasma arc)
39.1 (cement kiln)

	Nigeria
	CFC-12
	66.5 collected + 17.5 estimated 
	1.66 (domestic - rotary kiln)



· Replace Table 4 as follows:
	Country
	Destruction method
	Amount destroyed (mt)
	Cost-effectiveness (US $/kg)

	Colombia
	Domestic – HTI (rotary kiln)
	15.1a
	5.98-6.20b

	Georgia
	Export - HTI (France)
	1.47
	5.99c

	Ghana
	Export - HTI (Poland)
	1.27
	No cost data givend

	
	Export – HTI (the USA)
	1.0
	0.00e

	Mexico
	Domestic - argon plasma 
	74.1
	9.20f

	
	Domestic - cement kiln incineration
	39.1
	8.00f

	Nigeria
	Domestic – rotary kiln incineration
	1.66
	29.82f


a Total amount of liquid and gaseous ODS refrigerants as well as PU foams destroyed during test burns of the rotary kiln.
b Includes only net cost of destruction of liquid CFC-11 and gaseous CFC-12.
c Including all inland as well as maritime export transportation cost.
d No costs given as the amount of ODS waste was co-disposed with 5.2 mt of methyl bromide.
e Destruction costs covered by carbon credits at no cost to the project.
f Including cost of handling and in-country transportation.

· Replace paragraph 88 and Table 5 as follows:
88. Based on the analysis of the completion reports from the selected demonstration projects prepared by the project implementation teams, the projects resulted in emission reduction of 583,887 CO2‑equivalent tonnes. This amount was calculated based on the actual quantities and nature of ODS waste actually destroyed by the collective intervention of the five projects in the country reports for the second phase of the evaluation of the pilot demonstration projects on ODS disposal and destruction and shown in Table 5.

	Country
	Substance
	GWP*
	ODS destroyed (mt)
	Greenhouse gas emission reduction (CO2-eq. tonnes)

	Colombia
	CFC-11
	4,750
	2.75
	13,063

	
	CFC-12
	10,900
	0.78
	8,502

	
	CFC-11-based foam
	n/a
	5.98
	n/a

	
	HCFC-141b-based foam
	n/a
	5.59
	n/a

	 Subtotal
	15.10
	21,565

	Georgia
	CFC-12
	10,900
	1.47
	16,023

	 Subtotal
	1.47
	16,023

	Ghana
	CFC-12
	10,900
	2.27
	24,743

	Subtotal
	2.27
	24,743

	Mexico
	CFC-11
	4,750
	24.70
	117,325

	
	CFC-12
	10,900
	25.30
	275,770

	
	CFC-114
	10,000
	0.50
	5,000

	
	HCFC-22
	1,810
	40.10
	72,581

	
	HCFC-141b
	725
	0.20
	145

	
	HFC-134a
	1,430
	21.50
	30,745

	
	R-407
	2,107
	0.90
	1,896

	Subtotal
	113.20
	503,462

	Nigeria
	CFC-12
	10,900
	1.66
	18,094

	Subtotal
	1.66
	18,094

	Total for 5 projects
	133.70
	583,887


* Based on the IPCC 4th Assessment Report
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